1.2.2 | Connection mode alternatives

TAPI 170 connection modes to OpenScape Business

TAPI 170 can be used with a single system OpenScape Business or with networked OpenScape Business systems. TAPI 170 is connected via one OpenScape Business CSTA link.

TAPI 170 connection to a single OpenScape Business system

TAPI 170 communicates in the LAN with a single OpenScape Business system via a CSTA link. These following OpenScape Business models can be connected, the TAPI 170 functionality is identical:

TAPI 170 connected to OpenScape Business with Booster Card

TAPI 170 connected to OpenScape Business with Booster Server

TAPI 170 connected to OpenScape Business S (here with remote TSP functionality)

TAPI 170 connection to networked OpenScape Business systems

TAPI 170 communicates in the LAN with the OpenScape Business master system via CSTA link. TAPI 170 receives user information of other networked OpenScape Business systems via this CSTA link. TAPI 170 automatically receives information about an update of user parameters on the networked systems.

With operating TAPI 170 in a OpenScape Business network and connecting it to a OpenScape Business slave system, TAPI 170 only receives user information of this slave system.

You get further information about networked OpenScape Business systems in the OpenScape Business documentation.

TAPI 170 connected to networked OpenScape Business systems (here with remote TSP functionality)