1.3 | Requirements

Supported OpenScape Business models

The following OpenScape Business models are supported:

OpenScape Business model
CSTA interface
X3 (X3W and X3R)
Connection to a OpenScape Business basic system via UC Booster Card or UC Booster Server
X5 (X5W and X5R)
X8
S
integrated

Hardware requirements for the TAPI 170 PC

The TAPI 170 PC has to be network compatible and has to comply with the hardware requirements for the installed Windows version.

Released operation systems for the TAPI 170PC

| - | Windows Server 2008 R2

| - | Windows Server 2008 R2 with Terminal Server

| - | Windows Server 2012

| - | Windows Server 2012 with Terminal Server

| - | Windows Server 2016

| - | Windows Server 2016 with Terminal Server

| - | Windows Small Business Server 2011

| - | Windows Small Business Server 2012 (Windows 2012 Essentials)

These listed operation systems are released in virtual environments with VMware only. The existing Windows Server limits for the use of VMware apply. You find more information in the VMware documentation.

For more information please check the file readme.txt on the TAPI 170 installation CD.

For TAPI 170 on a telephony server PC with Terminal Server / Citrix please consider information given in the section TAPI 170 with Terminal Server / Citrix.

Software requirements for remote client PCs (with operation mode remote TSP)

• | 32-bit operation systems:

| - | Windows 7 (except Starter / Home Basic / Home Premium editions)

| - | Windows 8 / 10 (except Windows 8 RT)

• | 64-bit operation systems:

| - | Windows 7 (except Starter / Home Basic / Home Premium editions)

| - | Windows 8 / 10 (except Windows 8 RT)

The above listed operation systems are not released in virtual environments.

Other requirements

• | Network protocol: TCP/IP must be installed and activated.

• | The server and client PCs must be members of the same Windows domain.

• | NETBIOS must be activated for reading the MAC ID.

• | The server PC must have a fixed IP address (also when using DHCP).

• | Installation of TAPI 170 must be executed by an user with administration and domain administration rights.

• | For operation the telephone service on the server PC a user account with administration and domain administration rights is required.

• | File and printer sharing must be activated.

Used TAPI 170 IP port (default)

The CSTA link to OpenScape Business uses the IP port 8800 by default.

Restrictions

A parallel operation of TAPI 170 and TAPI 120 on the same telephony server is not possible. This limitation refers to both, OpenScape Business TAPI and HiPath TAPI.