3.2.2 | General parameters

To configure basic settings and the setup of the connection parameters to your OpenScape Business System you select the UC-Server tab.

Display

The General tab shows this parameters:

Parameter
Description
IP address of your Server
IP address of the connected OpenScape Business system determined during its installation and configuration.
IP port of the Server
IP port number of the OpenScape Business system. By default the port number is 8800.
Line devices
Select at least one type of Line devices (user type) to be monitored by TAPI 170 (controllable linedevice types). There are:
| - | Extensions
| - | Trunks
| - | UCD groups
After installation all devices are activated by default. For performance reasons please only select those line device types that are essentially required by the TAPI application (see also section Linedevice parameters).
CSTA user ID
Enter the CSTA user ID configured on the system. If the CSTA user ID is updated on the system, you have change it here accordingly.
CSTA user password
Enter the CSTA userpassword configured on the system. If the CSTA user password is updated on the system, you have change it here accordingly.
An input dialog opens in which you can enter and confirm the new password, then you return to the configuration dialog.

If this CSTA3 user password differs from the password in the systems WBM, the CSTA logon on the system is impossible!

Saving parameters

> | Click Apply to save entries without closing the dialog. e.g. to configure parameters in other tabs.
> | Click OK to save changes and to exit the configuration dialog.
> | A confirmation message appears in both cases, click Yes to save the parameter values. Your changes take effect after the Telephony Service on the TAPI PC has been restarted.