4 | Additional Configurations on the telephony server (remote TSP)

4.1 | General

User or client call numbers are made available for installing TAPI 170 during TAPI linedevice configuration (see Linedevice parameters). Using TAPI 170 with remote TSP these linedevices must be assigned with an additional configuration to the relevant users in the network. This ensures, that network subscribers can only use the linedevices reserved specifically for them.

The following description and figures are valid for Windows 2008 R2. For other Windows operation systems the description is valid accordingly.