3.2.4 | Linedevice parameters

The Linedevices tab

This tab shows all users (linedevices) of the connected system whose linedevice types correspond to the selected linedevice types for TAPI 170 monitoring (see section General parameters).

After initial installation of TAPI 170 no user is displayed. After start of a TAPI application or with click on Get Devices (this button is selectable with an empty list only) the referring linedevices are loaded to this list.

Display (after initial installation, empty list)

Display (with entries)

The list shows this parameters:

Column
Description
Call Number
Call number of the user, transmitted from the system
Line name
Line name of the user, transmitted from the system
Line device type
User line device type. This list shows only users with line device types that are selected for a monitoring by the TAPI application (see also section General parameters).

Saving parameters

> | Click Apply to save entries without closing the dialog. e.g. to configure parameters in other tabs.
> | Click OK to save changes and to exit the configuration dialog.
> | A confirmation message appears in both cases, click Yes to save the parameter values. Your changes take effect after the Telephony Service on the TAPI PC has been restarted.