5.1.1 | Entering the server name on the client PC

General

The telephony server name must be entered on every client PC to ensure proper communication between the client and server PC. Proceed as follows in the case of a client PC running Windows:

1. | Log on to Windows as a user with administration rights.

2. | Click Run in the Start menu.

3. | Enter the following command: TCMSETUP /C remoteserver where

| • | remoteserver is the name (not the IP address) of the telephony server PC.

You will be notified with a message box about the commands result (e.g. if the TAPI client is properly installed).